{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Blad1","Blad2","Blad3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Kunduppgifter"]
["Namn"]
["Adress"]
["Referens"]
["Datum"]
["Notering"]
[]
["Tillgänglig effekt/power supply",null,null,"Max maskin effekt",null,null,"Bestyckning Panel"]
[" ","230V16A P+N+E",null,"IH5 3,5 kVA ",null,null,"PC control"]
[null,"400V16A 3P+N+E",null,"IH10 11 kVA ",null,null,"PLC control"]
[null,"400V32A 3P+N+E",null,"IH18 22 kVA",null,null,"Temp control"]
[null,"400V32A 3P+N+E",null,"IH25 22 kVA",null,null,"Programfunktion"]
[" ","400V50A 3P+N+E",null,"IH30 30 kVA",null,null,"Effektreglering panel"]
[null,"400V63A 3P+N+E",null,"IH50 44 kVA",null,null,"Effektregl  handtag"]
[null,"400V125A 3P+N+E",null,"IH80 80 kVA"]
[]
["Kylning"]
["Processvatten"]
["Färskvatten",null,null,null,null," "," "]
["Fläktkylare",null,null,null,null,null,"Längd"]
["Kompressor",null,null,null,null,null," "]
["Annat",null,null,null,null,null," "]
[null,null,null,null,null,null," "]
[]
["Användning"]
["Lödning"]
["Smide",null,null,null,null,null,"Applikation"]
["Riktning",null,null,null,null,null,"Handtag med effektreglering"]
["Härdning",null,null,null,null,null,"Tryckknapp ON/OFF"]
["Värmning",null,null,null,null,null,"Maskinfäste fast montage"]
["Anlöpning",null,null,null,null,null,"Robothantering"]
["Smältning",null,null,null,null,null,"Annat"]
["Annat"]
[]
[null,null,null,"Dimension detalj",null,null,"Värmning data"]
["Material",null,null,"Vikt",null,null,"Cykeltid"]
["Stål",null,null,"ID",null,null,"Hålltid"]
["Cu/koppar",null,null,"YD",null,null,"Max temp"]
["Mässing",null,null,"B",null,null,"Min temp"]
["Grafit",null,null,"L",null,null,"Tid/temp ramp"]
["Annat",null,null,"H",null,null,"Övrigt"]

{"sheet":"Blad2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Blad3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}