{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Blad1","Blad2","Blad3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Customer Data"]
["Name"]
["Address"]
["Reference"]
["Date"]
["Note"]
[]
[null,"Power supply",null,"Max effect machine",null,null,"Contents Panel"]
[" ","230V16A P+N+E",null,"IH5 3,5 kVA ",null,null,"PC control"]
[null,"400V16A 3P+N+E",null,"IH10 11 kVA ",null,null,"PLC control"]
[null,"400V32A 3P+N+E",null,"IH18 22 kVA",null,null,"Temp control"]
[null,"400V32A 3P+N+E",null,"IH25 22 kVA",null,null,"Program function"]
[" ","400V50A 3P+N+E",null,"IH30 30 kVA",null,null,"Power control panel"]
[null,"400V63A 3P+N+E",null,"IH50 44 kVA",null,null,"Power control handle"]
[null,"400V125A 3P+N+E",null,"IH80 80 kVA"]
[]
["Cooling"]
["Process water"]
["Fresh water",null,null,null,null," "," "]
["Fan cooler",null,null,null,null,null,"Length"]
["Compressor",null,null,null,null,null," "]
["Other",null,null,null,null,null," "]
[null,null,null,null,null,null," "]
[]
["Usage"]
["Brazing"]
["Forging",null,null,null,null,null,"Application"]
["Strengthning",null,null,null,null,null,"Power control handle"]
["Hardening",null,null,null,null,null,"Push Botton ON/OFF"]
["Heating",null,null,null,null,null,"Machinefitting Fixed"]
["Annealing",null,null,null,null,null,"Robot Handling"]
["Melting",null,null,null,null,null,"Other"]
["Other"]
[]
[null,null,null,"Dimension detail",null,null,"Heating Data"]
["Material",null,null,"Weight",null,null,"Cycle Time"]
["Steel",null,null,"ID",null,null,"Hold Time"]
["Cupper",null,null,"OD",null,null,"Max temp"]
["Brass",null,null,"W ",null,null,"Min temp"]
["Graphite",null,null,"L",null,null,"Time/temp ramp"]
["Other",null,null,"H",null,null,"Other"]

{"sheet":"Blad2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Blad3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}